SDLT 220 SDLT 320 SDLT 600

300 | 36

110 | 11 160 | 16

Super DLTtape II

Super DLTtape I

Cleaning Tape III DLT VS DLT VS160 SDLT Cleaning Tape

Cleaning Tape Key

Super DLTtape II

Super DLTtape I

DLTtape VS1

DLTtape IV

DLTtape IIIXT

DLTtape III

DLT 2000XT

DLT 2000 DLT 4000 DLT 7000 DLT 8000 DLT VS160 SDLT 220 SDLT 320 SDLT 600

DLT VS80 DLT1

D R I V E S

M E D I A

20| 1.5 35| 5 40| 6 40| 3

300| 36

15| 1.5

110| 11

10| 1.25

160 | 16

80| 8

Optimum performance sample: The SDLT 600 uses Super DLTtape II, and has a native capacity of 300GB at 34 MB/sec transfer rate.

Compatibility sample: Start at the arrow below the drive and move left: • SDLT 600 is read compatibile with Super DLTtape I media written by the SDLT 320 and SDLT 220. • SDLT 320 using Super DLTtape I reads data written by SDLT 220 and writes in SDLT 220 mode.

Key

Optimum drive and media in shaded areas

Native capacity (GB) and transfer rate (MB per sec)

Compatibility information is found by starting at arrows

Read only compatible indicator

Read and write compatible indicator

DLTtape^™ Media Compatibility (Updated 10/22/03)