%%
%%

\section*{Supported Autochangers}
\label{_ChapterStart21}
\index[general]{Autochangers!Supported }
\index[general]{Supported Autochangers }
\addcontentsline{toc}{section}{Supported Autochangers}

\subsection*{Supported Autochangers}
\label{Models}
\index[general]{Autochangers!Supported }
\index[general]{Supported Autochangers }
\addcontentsline{toc}{subsection}{Supported Autochangers}

I hesitate to call these ``supported'' autochangers because the only
autochanger that I have in my possession and am able to test is the HP
SureStore DAT40X6. All the other autochangers have been reported to work by
Bacula users. Note, in the Capacity/Slot column below, I quote the Compressed
capacity per tape (or Slot). 

\addcontentsline{lot}{table}{Autochangers Known to Work with Bacula}
\begin{longtable}{|p{0.6in}|p{0.8in}|p{0.9in}|p{0.8in}|p{0.5in}|p{0.75in}|}
 \hline 
\multicolumn{1}{|c| }{\bf OS } & \multicolumn{1}{c| }{\bf Man. } &
\multicolumn{1}{c| }{\bf Media } & \multicolumn{1}{c| }{\bf Model } &
\multicolumn{1}{c| }{\bf Slots } & \multicolumn{1}{c| }{\bf Cap/Slot  } \\
 \hline 
{Linux } & {Adic } & {LTO-1/2, SDLT 320 } & {Adic Scalar 24 } & {24} & {100GB 
} \\
 \hline 
{Linux } & {Adic } & {LTO-2 } & {Adic FastStor 2, Sun Storedge L8 } & {8} &
{200GB  } \\
 \hline 
{- } & {Dell } & {LTO-2 } & {PowerValut 132T/136T } & {-} & {100GB  } \\
 \hline 
{Linux } & {Exabyte } & {VXA2 } & {VXA PacketLoader 1x10 2U } & {10} &
{80/160GB  } \\
 \hline 
{Linux Gentoo 1.4 } & {Exabyte } & {AIT-2 } & {215A } & {15 (2 drives)} &
{50GB  } \\
 \hline 
{Linux } & {HP } & {DDS-4 } & {SureStore DAT-40X6 } & {6 } & {40GB  } \\
 \hline 
{Linux } & {HP } & {Ultrium-2/LTO } & {MSL 6000/ 60030/ 5052 } & {28 } &
{200/400GB  } \\
 \hline 
{- } & {HP } & {DLT } & {A4853 DLT } & {30} & {40/70GB  } \\
 \hline 
{Linux } & {HP (Compaq) } & {DLT VI } & {Compaq TL-895 } & {96+4 import
export} & {35/70GB  } \\
 \hline 
{SuSE 9.0 } & {IBM } & {LTO } & {IBM 3581 Ultrium Tape Loader } & {7} &
{200/400GB  } \\
 \hline 
{- } & {Overland } & {LTO } & {Overland LoaderXpress LTO } & {10-19} & {100GB 
} \\
 \hline 
{- } & {Overland } & {LTO } & {Overland Neo2000 LTO } & {26-30} & {100GB  } \\
 \hline 
{FreeBSD 4.9 } & {QUALSTAR TLS-4210 (Qualstar) } & {AIT1: 36GB, AIT2: 50GB all
uncomp } & {QUALSTAR TLS-4210 } & {12} & {AIT1: 36GB, AIT2: 50GB all uncomp  }
\\
 \hline 
{Linux } & {Skydata } & {DLT  } & {ATL-L200 } & {8} & {40/80  } \\
 \hline 
{-  } & {Sony  } & {DDS-4 } & {TSL-11000 } & {8} & {40GB  } \\
 \hline 
{Linux } & {Sony  } & {AIT-2 } & {LIB-304(SDX-500C) } & {?} & {200GB  } \\
 \hline 
{FreeBSD 4.9-STABLE } & {Sony } & {AIT-1 } & {TSL-SA300C } & {4} & {45/70GB  }
\\
 \hline 
{- } & {Storagetek } & {DLT } & {Timberwolf DLT } & {6} & {40/70  } \\
 \hline 
{Solaris } & {Sun } & {4mm DLT } & {Sun Desktop Archive Python 29279 } & {4} &
{20GB  } \\
 \hline 
{Linux } & {Tandberg } & {DLT VI } & {VS 640 } & {8?} & {35/70GB  } \\
 \hline 
{Linux 2.6.x } & {Tandberg Data } & {SLR100 } & {SLR100 Autoloader } & {8} &
{50/100GB }
\\ \hline 

\end{longtable}

